Solution to redmine 5905

 sSrvN4 allow reject as well

August 24, 2022

sSrvN4 both an error message and reject from device that does not support SetDataValues should be considered "pass".

|  |  |  |
| --- | --- | --- |
| **sSrvN4** | **SetDataValues of read-only FCDA** | [ ]  Passed[ ]  Failed[ ]  Inconclusive |
| IEC 61850-7-2 Subclause 11.4.3IEC 61850-8-1 Subclause 8.1.3.4.4.2, Table 23 |
| Expected result1. DUT sends response with data access error “object-access-denied” or a reject
 |
| Test description1. Client sends a SetDataValues request with a read-only FCDA
 |
| Comment |