Solution to redmine 5905

sSrvN4 allow reject as well

August 24, 2022

sSrvN4 both an error message and reject from device that does not support SetDataValues should be considered "pass".

|  |  |  |
| --- | --- | --- |
| **sSrvN4** | **SetDataValues of read-only FCDA** | Passed  Failed  Inconclusive |
| IEC 61850-7-2 Subclause 11.4.3  IEC 61850-8-1 Subclause 8.1.3.4.4.2, Table 23 | | |
| Expected result   1. DUT sends response with data access error “object-access-denied” or a reject if MMS write service supported bit is false. | | |
| Test description   1. Client sends a SetDataValues request with a read-only FCDA | | |
| Comment | | |