Solution to redmine 6198

**How to interpret SCL with Services element in the IED and in the AccessPoint?**

December 16, 2022

Update Server test procedure to add new sCnf66

### A2.5 SCL IED Services section

|  |  |  |
| --- | --- | --- |
| **Test case** | **Test case description** | **Verdict** |
| sCnf66 | Verify that Services are not defined at IED and AccessPoint levels at the same time, except for ConfReportControl.max, GOOSE.max and SMVsc.max wchic may be overwritten only with value 0 indicating the deactivation of the service for a specific AccessPoint. | Passed  Failed  Inconclusive |

Update Client test procedure to add new sCnf7

**A2 Configuration file (IEC 61850-6)**

ICD export test procedures

|  |  |  |
| --- | --- | --- |
| **Id** | **Test procedure** | **Verdict** |
| cCnf6 | Verify that Services are not defined at IED and AccessPoint levels at the same time. |  |