Solution to redmine 6541

### Use same dataset in URCB, BRCB and GoCB

Dec 19, 2023

|  |  |  |
| --- | --- | --- |
| sCnf5 | Import the ICD or IID file from sCnf4 into SCT SIMULATOR and generate SCD file (when supported):  - set IED name  - add or update datasets  - add or update unbuffered and buffered report control blocks  - add or update GOOSE control blocks and MAC address  - **use the same dataset in at least one URCB, BRCB and GoCB**  - add or update SV control block(s) and MAC address  - subscribe to data flows from other IED’s  Import the SCD file into the ICT tool and select the IED to be handled from IED’s named in the SCD file by IED name | Passed  Failed  Inconclusive |