Solution to redmine #658

May 21, 2021

New test case:

|  |  |  |
| --- | --- | --- |
| **cRpXX** | **Process a report before the enable response** | **Passed**  **Failed**  **Inconclusive** |
| IEC 61850-7-2 clause 17.2  IEC 61850-8-1 clause 17.1, 17.2  *PIXIT Rp8* | | |
| Expected result   1. DUT successfully configures and enables the report control block 2. The DUT processes the report with the new value as normal | | |
| Test description   1. Force the DUT to Configure and enable an URCB which a valid data set 2. Force the SERVER SIMULATOR to send a report with a new data value **before** the enable response | | |
| Comment | | |

Add this test case to the certificate and table A4.2 as mandatory,