Solution to redmine #658

May 21, 2021

New test case:

|  |  |  |
| --- | --- | --- |
| **cRpXX** | **Process a report before the enable response**  | **Passed****Failed****Inconclusive** |
| IEC 61850-7-2 clause 17.2IEC 61850-8-1 clause 17.1, 17.2*PIXIT Rp8* |
| Expected result1. DUT successfully configures and enables the report control block
2. The DUT processes the report with the new value as normal
 |
| Test description1. Force the DUT to Configure and enable an URCB which a valid data set
2. Force the SERVER SIMULATOR to send a report with a new data value **before** the enable response
 |
| Comment |

Add this test case to the certificate and table A4.2 as mandatory,