Solution to redmine #658

May 21, 2021

New test case:

|  |  |  |
| --- | --- | --- |
| **cRpXX** | **Process a report before and after the enable response**  | **Passed****Failed****Inconclusive** |
| IEC 61850-7-2 clause 17.2IEC 61850-8-1 clause 17.1, 17.2*PIXIT Rp8* |
| Expected result1. DUT successfully configures and enables the report control block
2. The DUT processes the report with the new value as normal
3. The DUT processes the report with the new value as normal
 |
| Test description1. Force the DUT to Configure and enable an URCB which a valid data set
2. Force the SERVER SIMULATOR to send a report with a new data value **before** the enable response
3. Force the SERVER SIMULATOR to send a report with a new data value **afer** the enable response
 |
| Comment |

Add this test case to the certificate and table A4.2 as mandatory,

Same for BRCB.