Solution to redmine #658

May 21, 2021

New test case:

|  |  |  |
| --- | --- | --- |
| **cRpXX** | **Process a report before and after the enable response** | **Passed**  **Failed**  **Inconclusive** |
| IEC 61850-7-2 clause 17.2  IEC 61850-8-1 clause 17.1, 17.2  *PIXIT Rp8* | | |
| Expected result   1. DUT successfully configures and enables the report control block 2. The DUT processes the report with the new value as normal   4. The DUT processes the report with the new value as normal | | |
| Test description   1. Force the DUT to Configure and enable an URCB which a valid data set 2. Force the SERVER SIMULATOR to send a report 3. SERVER SIMULATOR sends the enable response 4. Force the SERVER SIMULATOR to send another report with a different new data value | | |
| Comment | | |

Add this test case to the certificate and table A4.2 as mandatory,

Same for BRCB.