Solution to redmine #6471

August 21, 2023

Part 8-1 Ed1 $20.4.2 states: the Select Response+ is a non-NULL value for the SBO attribute.

Update sSBOns10

|  |  |  |
| --- | --- | --- |
| **cSBOns10** | **Select and successful Operate on Ed1 server** | 🞎 Passed  🞎 Failed  🞎 Inconclusive |
| IEC 61850-7-2 clause 20.2.2, 20.5.3.5  IEC 61850-8-1 clause 20.8 | | |
| Expected result  1. The DUT sends a correct Select request for the SBOns object and accepts the SBO value  2. The DUT sends a correct Operate request on the selected SBOns object | | |
| Test description   1. Force the DUT to perform a Select request on an SBOns object in an Ed1 server, the SERVER   SIMULATOR responds with SBO any value not matching <CO\_ CtrlObjectRef>, e.g. the <CO\_ CtrlObjectRef>with tailing SBO or Oper  2. Force the DUT to perform an Operate request on the selected SBOns object | | |
| Comment | | |