Solution to redmine #6471

August 21, 2023

Part 8-1 Ed1 $20.4.2 states: the Select Response+ is a non-NULL value for the SBO attribute.

Update sSBOns10

|  |  |  |
| --- | --- | --- |
| **cSBOns10** | **Select and successful Operate on Ed1 server** | 🞎 Passed🞎 Failed🞎 Inconclusive |
| IEC 61850-7-2 clause 20.2.2, 20.5.3.5IEC 61850-8-1 clause 20.8 |
| Expected result1. The DUT sends a correct Select request for the SBOns object and accepts the SBO value2. The DUT sends a correct Operate request on the selected SBOns object |
| Test description1. Force the DUT to perform a Select request on an SBOns object in an Ed1 server, the SERVER

 SIMULATOR responds with SBO any value not matching <CO\_ CtrlObjectRef>, e.g. the <CO\_ CtrlObjectRef>with tailing SBO or Oper2. Force the DUT to perform an Operate request on the selected SBOns object |
| Comment |