|  |  |  |
| --- | --- | --- |
| **Test case** | **Test case description** | **Verdict** |
| sCnf10 | Verify the ICD has at most one Substation or Line or Process exists at SCL level and the attribute “name” is “TEMPLATE”. ~~If voltagelevel and bay element are present, their name is “TEMPLATE”~~Condition: when substation section is present | [ ]  Passed[ ]  Failed[ ]  Inconclusive[ ]  Not applicable |