Solution to redmine 748 sGos9

|  |  |  |
| --- | --- | --- |
| **sGos9** | **Subscribe GOOSE message with “fixed length” GOOSE** | Passed  Failed  Inconclusive |
| IEC 61850-7-2 Subclause 18.2.3  IEC 61850-8-1 Subclause A.3  PIXIT Gs8 | | |
| Expected result   1. DUT updates the value and sends a GOOSE message with changed integer value 2. DUT updates the value and sends a GOOSE message with changed integer value | | |
| Test description  Test engineer configures the DUT with subscribed GOOSE (ping-pong mechanism) containing a “Beh.stVal” or an integer value or a Boolean value  When INS or ENS subscribe is supported   1. Publisher sends “fixed length” GOOSE with initial integer value 2. Publisher sends “fixed length” GOOSE with other integer value   When INS subscribe is not supported   1. Publisher sends “fixed length” GOOSE with initial boolean value 2. Publisher sends “fixed length” GOOSE with other boolean value | | |
| Comment | | |