Solution to redmine 748 sGos9

|  |  |  |
| --- | --- | --- |
| **sGos9** | **Subscribe GOOSE message with “fixed length” GOOSE** | [x]  Passed[ ]  Failed[ ]  Inconclusive |
| IEC 61850-7-2 Subclause 18.2.3IEC 61850-8-1 Subclause A.3PIXIT Gs8 |
| Expected result1. DUT updates the value and sends a GOOSE message with changed integer value
2. DUT updates the value and sends a GOOSE message with changed integer value
 |
| Test descriptionTest engineer configures the DUT with subscribed GOOSE (ping-pong mechanism) containing a “Beh.stVal” or an integer value or a Boolean valueWhen INS or ENS subscribe is supported1. Publisher sends “fixed length” GOOSE with initial integer value
2. Publisher sends “fixed length” GOOSE with other integer value

When INS subscribe is not supported1. Publisher sends “fixed length” GOOSE with initial boolean value
2. Publisher sends “fixed length” GOOSE with other boolean value
 |
| Comment |